Top > INSTALLATION > Before Installation > Ambient Temperature

## Ambient Temperature

- The appliance is designed to operate within a limited range of ambient temperatures, depending on the climate zone.

- The internal temperatures could be affected by the location of the appliance, the ambient temperature, the frequency of door opening and so on.

- The climate class can be found on the rating label.

Climate Class | Ambient Temperature Range ºC
--- | ---
SN (Extended Temperate) | +10 - +32
N (Temperate) | +16 - +32
ST (Subtropical) | +16 - +38 / +18 - +38**
T (Tropical) | +10 - +43* / +16 - +43 / +18 - +43**

* Australia, India, Kenya

** Argentina

Note

- The appliances rated from SN to T are intended to be used at an ambient temperature between 10 ºC and 43 ºC.