Top > INSTALLATION > Before Installation > Dimensions and Clearances

## Dimensions and Clearances

Too small of a distance from adjacent items may result in the degradation of freezing capability and increased electricity costs. Allow over 50 mm of clearance from each adjacent wall when installing the appliance.

| a | b
--- | --- | ---
| Size (mm)
A | 595 | 595
B | 1 720/1 860/2 030 | 1 720/1 860/2 030
C | 682 | 677/675
D | 615 | 610
E | 682 | 677/675
F | 1 230 | 1 225
G | 995 | 995
H | 2 200 | 2 200

Note

- The measurements in the table above are approximate.

- You can determine what type of appliance it is by looking at the label inside the appliance.